Max length = 100

Max dia = 4.5

Stability between 3 and 4

With motor (F15) => total wt 750 g

Use load of 100g or use a bulk head and assign a mass 100 g